Four-post lift 5t, 400V

Reference: STD-5650

The Lincos STD-5650 four-post lift, with a capacity of 5 tonnes, enables fast, convenient and safe vehicle maintenance. The lifting height is 1700 mm. Has an auxiliary lift for a more accurate inspection and easier access, as well as sliding plates for wheel alignment.

**Description**

* Electro hydraulic four-post lift for repair and maintenance of vehicles in every workshop.
* The lift is also suitable for wheel alignment.
* It contains sliding plates and 2 ramps.

**Electrohydraulic auxiliary lift**

* Allows more detailed inspection and easier access (electrohydraulic channel lift)
* Lifting height: 340mm.
* Load capacity: 2.5 ton.

**Technical description:**

|  |  |
| --- | --- |
| Lift capacity | 5000kg |
| Maximum raised height | 1700mm |
| Runway length | 5000mm |
| Runway width | 580mm |
| Free width between runways | 880/960mm |
| Width between two columns | 2880mm |
| Overall length | 5825mm |
| Overall height | 2220mm |
| overall width | 3286mm |
| Raised time | 60s |
| Noise level | 75dB(A)/1m |
| Working temperature | 0°C - 40°C |
| Motor voltage | 380V / 220V |
| Motor power | 2.2KW |
| Weight | 1480kg |

### SHIPPING PARAMETERS

|  |  |
| --- | --- |
| **Product weight** | 1 475.00kg |
| **Width** | 64.00cm |
| **Depth** | 123.00cm |
| **Height** | 510.00cm |